Solmeta GMAX-EOS Ver1.2 (2017-01-10) for Canon cameras  

The Ver1.2 is an upgrade from Ver1.1. This is the second released version. 

1/ Trouble shoot a bug about Log function.
ON [Auto] mode, when shoot a picture, the log record can not been wrote into 4GB flash card by hot shoe trigger. Now Ver1.2 works well.

2/ Find some brands 4GB flash card writing data not stable.
When use Toshiba flash card, in some special case, GMAX-EOS writes log data into this card failed. Now Ver1.2 works stable.



Solmeta INC.
Jan.10, 2017

-----------------------------------------------------------------
Solmeta GMAX-EOS Ver1.1 (2016-12-01) for Canon cameras 
This is the first release version.

Solmeta INC.
Dec.01, 2016
