Solmeta GMAX-EOS V1.5 Release 20180112 for Canon cameras



The Ver1.5 is a release version from Ver1.3. This is the 4rd released version.

The firmware file name is "GMAX-EOS V1.5 (without bluetooth function) Release 20180112.dfu"

1. This version is for GMAX-EOS without bluetooth remote shutter release hardware function. If you have a GMAX-EOS+ with bluetooth remote function, please download the Ver1.5+ firmware.

2. Improve hot-shoe link communication long time stable feature, especially for Canon EOS80D camera.

3. Improve USB cable link communication long time stable feature, especially for Canon EOS80D camera.

4. Trouble shoot a bug which cause EOS80D camera dead (have to do power off/ on for the camera)

5. Trouble shoot a bug which -12 to -1 TimeZone set can not be saved on the last version 1.3

6. Trouble & improve some other little bugs which users can not feel.




SOLMETA CO., LTD
Jan. 12, 2018











Solmeta GMAX-EOS V1.3 Release 20170429 for Canon cameras
The Ver1.3 is an upgrade from Ver1.2. This is the 3rd released version. 
The new firmware file name is ¡°GMAX-EOS V13 Release 20170429.dfu¡±
1. A professinal user named Bill and another user named Hendrik report to us that they find a bug at the same time:
On the log file the three sentences $GPRMC,$PTNTHPR and $GPGGA have wrong checksums, so some software can not use these sentences.
We find there is a bug on these three sentences's checksums.
We upgrade and trouble shoot the bug.
2. We add a sentence $GPGSA on the log files, so there are 4 sentence on the log files.

We release this version Ver1.3.
If you do not care the GMAX-EOS's log files, you can keep in Ver 1.2, no other problem.


SOLMETA CO., LTD
May 12, 2017





Solmeta GMAX-EOS Ver1.2 (2017-01-10) for Canon cameras  

The Ver1.2 is an upgrade from Ver1.1. This is the second released version. 

1/ Trouble shoot a bug about Log function.
ON [Auto] mode, when shoot a picture, the log record can not been wrote into 4GB flash card by hot shoe trigger. Now Ver1.2 works well.

2/ Find some brands 4GB flash card writing data not stable.
When use Toshiba flash card, in some special case, GMAX-EOS writes log data into this card failed. Now Ver1.2 works stable.



Solmeta INC.
Jan.10, 2017

-----------------------------------------------------------------
Solmeta GMAX-EOS Ver1.1 (2016-12-01) for Canon cameras 
This is the first release version.

Solmeta INC.
Dec.01, 2016
